|  |  |
| --- | --- |
| CATEGORY: | CYLINDRICAL GRINDING MACHINE |
| Manufacturer: | BERCO |
| Model: | RUY 300/3000 |
| Centre height | 300 mm / 11 13/16” |
| Centre distance | 3000 mm / 118 7/64” |
| Mandrel rotating speeds (n. 12) | from 14 to 220 |
| Max grinding diameter | 600 mm / 23 5/8” |
| Wheel centre head stroke (fast) | 50 mm / 1 31/32” |
| Wheel centre head stroke (fast) | 150 mm / 5 29/32” |
| Grinding wheel max diameter | 650 mm / 25 19/32” |
| Max table tilt | 3° 30′ |
| Total power | 27,7 HP |
| Dimensions | 7100 x 2300 mm / 23.35 Ft x 7.65 Ft |
| Approximate weight | 11800 kg / 26,014 lbs |
|  |  |

****

**BERCO RUY 300/3000 GRINDING MACHINE**